The logic design comprises of three sub logic units:

1. Converting the input taken from the keyboard (ASCII value) to the hexadecimal value to provide it to the memory unit.

2. Memory unit for the address generation. It contains addresses for 16 valid inputs + 1 address for the invalid input.

3. Enabler circuit logic for the left to right column wise implementation of the LED matrix.